**PinPoint Software Update Procedure**

*3.1.15 WNK*

The PinPoint thumb drives that are supplied with each system should be used to load the software. The file names of the software must not be changed. Only one version of CapView, PowerHub, and VCM software must be loaded on the root directory of the PinPoint thumb drive. The instructions below are for a complete software update.

Instructions to perform software update:

1. Turn on the CapView.
2. **Record all system, location, and nozzle settings.**
3. Insert the thumb drive with software on root directory in CapView.
4. The CapView will display options for updating the components that have software present on the thumb drive.
5. **The CapView must be updated first**. Install software on CapView – lights will blink while it is updating, it will shut off when finished
6. Turn on CapView.
7. Install software on PowerHub – blue bar will appear on screen to show update progress. Will return to main update screen when complete.
8. Install software on VCMs – blue bar will appear on screen to show update progress. Will return to main update screen when complete.
9. Turn off CapView and **remove thumb drive.**
10. Turn on CapView.
11. Perform a Factory reset (found in system setup menu). CapView will automatically shut down.
12. **Wait 5 minutes** then turn on CapView.
13. All Location setup, system setup and nozzle setup information must be re-entered.